# pico-temp-controller

pid temperature controller using the pi pico.

## steps:
* learn RTIC, get 2 leds blinking at two different rates, and an led toggling on button press with interrupts.
* learn to interface with i2c, print temperature measurements to serial
* learn to interface with rotary encoder, print rotation directions to serial.
* learn to interface with lcd, print temp measurements and rotation to lcd.
* develop pid loop to control solid state relay, with temp from temp sensor and target temp from rotary encoder.

## crates to use:
[thermocouple chip](https://crates.io/crates/max31855)
[lcd](https://crates.io/crates/lcd)
[rotary encoder](https://crates.io/crates/rotary-encoder-embedded)
